READ ME - File name details 

Model - Airflow - Mounting type - Coil Hand - Coil

Model - RCW - ceiling or wall type
Model - RCWI - ceiling or wall type inverted airflow
Model - RFF - floor mounted
Model - RFFI - floor mounted inverted airflow
Model - RFS  - floor mounted slope top
Model - RFSI - floor mounted slope top inverted

Airflow -ceiling/wall 380, 400, 420, 430, 290, 300, 350
Airflow - floor - 200, 220, 240, 250
	Denotes inlet and outlet location, see drawings for details

Mounting type - R - Recessed
Mounting type - E - Exposed
	RCW units only, all floor units are exposed

Coil hand - L - LH coil connection
Coil hand - R - RH coil connection

Coil - 1 row
Coil - 2 row
Coil - 4 row


